

**4000BPH(for 500ml bottle) Juice Filling Line Quotation**

|  |  |  |  |
| --- | --- | --- | --- |
| **Pure Water Treatment System** | | | |
| 1 | Pure Water Treatment Machine | GRA-1000I(2000L/H) | 1pcs |
| 2 | CIP Cleaning system | 1pcs |
| 3 | Water tanks(SUS304) | 2T | 2pcs |
| 4 | Ozone System | 6G | 1pcs |
| 5 | UV System | 40W | 1pcs |
| **Beverage System** | | | |
| 1 | Melting sugar pot | DHT-500 | 2pcs |
| 2 | Hot resist Beverage pump | 3000L/H | 1pc |
| 3 | Syrup filter | TML-500 | 2pcs |
| 4 | Preparation tank(hot/cold, double layer ) | JB-1000L | 1pcs |
| 5 | Double-Joint filters | 2T | 1pcs |
| 6 | Vacuum Degasser | 1000l/h | 1pcs |
| 7 | Double screw pumps | 2000L/H | 1pcs |
| 8 | **High Temperature Instantaneous Sterilizer** | UHT-2000 | 1pcs |
| 9 | Hot preserve tank | 2000L | 1pcs |
| 10 | CIP Cleaning system | CIP-500(semi) | 1pcs |
| 11 | Pipes etc | SUS304 | 1lot |
| **Automatic Juice Filling Line** | | | |
| 1 | Automatic Hot Filling Machine(monoblock) | GRA 14-12-5 | 1pcs |
| 2 | Light inspection | 1pcs | Free |
| 3 | Conveyor system(Including motors,sensors) | 10M |  |
| 4 | **Bottle overturn sterilizer** | DP-6 | 1pcs |
| 5 | **Water Spray bottle cooling machine** | PL-6 | 1pcs |
| 6 | Bottle body drying machine | CG-1 | 1pcs |
| 7 | Automatic Labeling machine by double driving labeling system | | |
| 8,1 | Automatic label wrapper | GRA-TB(150A) | 1pcs |
| 8,2 | Label shrink tunnel |  | 1pcs |
| 8,3 | Steam generator |  | 1pcs |
| 9 | Laser printer | 10W | 1pcs |
| 10 | Automatic shrinking wrapping machine |  |  |
| 10,1 | Automatic Film Wrapper | GRA-MB(150) | 1pcs |
| 10,2 | Heating shrinking tunnel |  | 1pcs |
| 10,3 | Air compressor |  | 1pcs |
| 11 | Extra Full bottle conveyor |  | 10M |
| **Automatic Blower for hot resist Bottles** | | | |
| 1 | Servo Automatic blow machine | 1pcs | 4 cavities |
| 2 | Preform unscrambler and lifting machine | 1pcs | By servo control |
| 3 | Win Industrial Chilling water machine:5HP | 1pcs | 5HP, LJ-05wi |
| 4 | Bottle mold(500ml,4cavities) | 1pcs | Aluminium |
| 5 | Mould temperature controller | 1pcs |  |
| 6 | Hengda Air compressor:WH-2.2/30 |  |  |
| 7 | High pressure Air compressor,2.2M3/40bar | 2pcs | Hengda brand |
| 8 | High Pressure air storage tank:1m3/34bar | 1pcs | SUS304 |
| 9 | Air Filters | 4pcs |  |
| 10 | High pressure Air Dyer | 1pcs |  |

****